; name and version number:@(#)cpqwav16.inf	1.1*/
; date of get: 		  08/18/98 13:30:15*/
; date of delta:	  11/14/97 14:38:47*/
; Copyright 1997, Compaq Computer Corporation.  All rights reserved.
; Copyright 1997 Lucent Technologies
;
; Modem Audio information file for Compaq Presario Modem
;
; Last Revised: 10/23/97

[Version]
Signature="$CHICAGO$"
Class=MEDIA
provider=%PROV%

[ClassInstall]
Addreg=Class.AddReg

[Class.AddReg]
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[Manufacturer]
%MfgName%=Microsoft

[Microsoft]
; the device id's (MODEMWAVE\LT_Win_Modem)
; correspond EXACTLY to the modem name with underscores in place of spaces.
; the names must be an exact match or installer won't find device.
; this scheme is because of the way the serial wave device enumeration occurs.

; serial wave device - imaadpcm driver
%Serial.DeviceDesc%=MSSERWAVE, MODEMWAVE\Compaq_Armada_1500_Series_560CL

[PreCopySection]
HKR,,NoSetupUI,,1

[MSSERWAVE]
AddReg=MSSERWAVE.AddReg

[MSSERWAVE.AddReg]
HKR,,DevLoader,,mmdevldr.vxd
HKR,Drivers,MIGRATED,,0
HKR,Drivers\wave,,,
HKR,,Driver,,serwave.vxd
HKR,Drivers\wave\serwvdrv.drv,Description,,%Serial.DeviceDesc%
HKR,Drivers\wave\serwvdrv.drv,Driver,,serwvdrv.drv
HKR,Drivers,SubClasses,,"wave"
HKR,Config,XformModule,  , "umdmxfrm.dll"
HKR,Config,XformID,     1, 04, 00, 00, 00
HKR,Config,BaudRate,	1, 00, c2, 01, 00
; 2 wave devices - line & local phone
;HKR,Config,WaveDevices,  1, 02, 00
; 1 wave device - only line
HKR,Config,WaveDevices,  1, 01, 00

;---------------------------------------------------------------;

[Strings]
PROV="Compaq"
MfgName="Compaq"
Serial.DeviceDesc="Voice Modem Serial Wave Device"
MediaClassName="Sound, video and game controllers"

