[attributes]

MODELS=Compaq Armada 56K (V.90) Modem
NULL MODEM=0
MAXIMUM SPEED=57600
DEFAULT SPEED=57600

FIXED SPEED=0
VER=100

[cc:Commands]
CCSETUP= 
BLIND DIAL=ATX1 
ANSWER RINGS OFF=ATS0=0
ANSWER RINGS ON=ATS0=1
CCHANGUP=
MODEM BUFFER=52
 

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0V1
SETUP=ATQ0&D2&C1S0=0S7=60X4
VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
RTS/CTS ENABLED=AT&K3
RTS/CTS IGNORED=AT&K0
ANSWER=ATA
MANUAL DIAL=ATX3S9=1D,
AUTO DIAL SETUP=ATS9=6
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]
OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER
NO CARRIER=NO CARRIER
NO DIALTONE=NO DIALTONE
NO DIALTONE=NO DIAL TONE

ERROR=ERROR
RING=RING

CONNECT, 115200=CONNECT 115200
CONNECT,  57600=CONNECT 57600
CONNECT,  38400=CONNECT 38400
CONNECT,  33600=CONNECT 33600
CONNECT,  31300=CONNECT 31300
CONNECT,  28800=CONNECT 28800
CONNECT,  26400=CONNECT 26400
CONNECT,  24000=CONNECT 24000
CONNECT,  21600=CONNECT 21600
CONNECT,  19200=CONNECT 19200
CONNECT,  16800=CONNECT 16800
CONNECT,  14400=CONNECT 14400
CONNECT,  12000=CONNECT 12000
CONNECT,   9600=CONNECT 9600
CONNECT,   7200=CONNECT 7200
CONNECT,   4800=CONNECT 4800
CONNECT,   2400=CONNECT 2400
CONNECT,   1200=CONNECT 1200
CONNECT,    600=CONNECT 600
CONNECT,    300=CONNECT 

