[attributes]

MODELS=COMPAQ ARMADA 56K (V.90) MODEM
NULL MODEM=0
MAXIMUM SPEED=115200
DEFAULT SPEED=115200

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&FE0W1&C1&D2S95=44
RTS/CTS ENABLED=AT&K3&R0
RTS/CTS IGNORED=AT&K0&R1
VOLUME OFF=ATM0
VOLUME LOW=ATM1L0
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX3S9=1D
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK
BUSY=BUSY
NO ANSWER=NO ANSWER
NO CARRIER=NO CARRIER
NO DIALTONE=NO DIALTONE
ERROR=ERROR
RING=RING

CONNECT, 115200=CONNECT 115200*
CONNECT, 57600=CONNECT 57600*
CONNECT, 38400=CONNECT 38400*
CONNECT, 19200=CONNECT 19200*
CONNECT, 14400=CONNECT 14400*
CONNECT, 12000=CONNECT 12000*
CONNECT,  9600=CONNECT 9600*
CONNECT,  7200=CONNECT 7200*
CONNECT,  4800=CONNECT 4800*
CONNECT,  2400=CONNECT 2400*
CONNECT,  1200=CONNECT 1200*

CARRIER,,28800=CARRIER 28800*
CARRIER,,26400=CARRIER 26400*
CARRIER,,24000=CARRIER 24000*
CARRIER,,21600=CARRIER 21600*
CARRIER,,19200=CARRIER 19200*
CARRIER,,16800=CARRIER 16800*
CARRIER,,14400=CARRIER 14400*
CARRIER,,14400=CARRIER 14000*
CARRIER,,12000=CARRIER 12000*
CARRIER,, 9600=CARRIER 9600*
CARRIER,, 7200=CARRIER 7200*
CARRIER,, 4800=CARRIER 4800*
CARRIER,, 2400=CARRIER 2400*
CARRIER,, 1200=CARRIER 1200*
