README.TXT

-----------------------------------------------------------------------
Compaq Armada 56K (V.90) Modem
SP9449.EXE  Version 1.0   01/25/99
-----------------------------------------------------------------------


Introduction:

This diskette contains the script files needed to support the following
applications:

- Lotus Notes 3.2x and later
- Lotus cc:Mail 7.0
- Microsoft MS-Mail 3.2 Remote


Contents:

A) Installing the Lotus Notes script file (CPQLN56K.MDM)
B) Installing the cc:Mail 7.0 script file (CPQCC56K.MDM)
C) Installing the Microsoft MS-Mail 3.2 script file (CPQMS56K.SCR)

-----------------------------------------------------------------------

A) Installing the Lotus Notes script file
   
***********************************************************************
(note: these instructions are based on Lotus Notes 4.x versions.
       Installation procedures may differ with older versions.  Consult
       your user's manual for script installation instructions.)
***********************************************************************

   1. Copy the CPQLN56K.MDM file to the \NOTES\DATA\MODEMS directory.
   2. Open the Lotus Notes program and click on File/Tools/User Preferences
      from the menu bar.
   3. In the User Preferences dialog box, click on the 'Ports' icon.
   4. Make sure the COM port the modem is located is selected and that the 'Port Enabled' checkbox
      is checked.
   5. Click on the 'COMx Options' button.
   6. In the Additional Setup dialog box, click on the 'Modem Type'
      drop-down list and select the "Compaq Armada 56K (V.90) Modem"
      entry.
   7. Make sure the following options are set:
        - maximum port speed = 115200
        - port number = modem COM port number
        - hardware flow control is checked
   8. Click on OK to close the Additional Setup dialog box, and close
      all remaining dialog boxes.

-----------------------------------------------------------------------

B) Installing the cc:Mail 7.0 script file
   
   1. Consult your user's manual for script installation.

-----------------------------------------------------------------------

C) Installing the Microsoft MS-Mail 3.2 Remote script file
   
   1. Copy the CPQMS56K.SCR file to the C:\WINDOWS\MS-Mail\MSRMT\GLB directory.
   2. Open the MS-Mail Remote application and click on the 'Mail' option on
      the menu bar and then select 'Communications'.
   3. In the 'Script' drop-down menu, select the "Compaq Armada 56K (V.90) Modem" 
      entry from the modem list.
   4. In the 'Communication' dialog, make sure that the baud rate is set to
      57600 and the port is set to modem COM port number.
   5. Click OK to close the dialog box

 -----------------------------------------------------------------------
